1. **GENERAL**
   1. **Related BCIT Guidelines**
      1. Section 06 46 00 Architectural Woodwork.
2. **DESIGN REQUIREMENTS**
   1. **Seismic**
      1. Provide seismic restraint for all shelving.
      2. Provide seismic restraint for all freestanding cabinets taller than 1200 mm.

\*\*\* END OF **FABRICATED CASEWORK** SECTION \*\*\*