1. **GENERAL**
	1. **Related BCIT Guidelines**
		1. Section 06 46 00 Architectural Woodwork.
2. **DESIGN REQUIREMENTS**
	1. **Seismic**
		1. Provide seismic restraint for all shelving.
		2. Provide seismic restraint for all freestanding cabinets taller than 1200 mm.

\*\*\* END OF **FABRICATED CASEWORK** SECTION \*\*\*