1. **GENERAL**
   1. **Requirements Include**
      1. Finish slabs-on-grade, monolithic suspended floor slabs, and concrete toppings.
      2. Include surface treatment with concrete hardener and sealer.
   2. **Related BCIT Guidelines**
      1. Section 03 30 00 Cast-in-Place Concrete.
      2. Section 07 92 00 Joint Sealants.
   3. **Design Requirements**
      1. Verify with Owner the level of grind or concrete and gloss of floor if any.
2. **PRODUCTS**
   1. **Performance**
      1. Flooring finish shall be durable and low maintenance.
      2. Flooring finish must meet low VOC requirements.
   2. **Materials**
      1. Concrete Densifier/Hardener.
      2. Sealer.

\*\*\* END OF **CONCRETE FINISHING** SECTION \*\*\*